**AIRCRAFT SALES BULLETIN**

MILITARY MODEL UH-1H

FOR SALE AIRWORTHY

|  |  |  |
| --- | --- | --- |
| SERIAL NUMBER | MANUFACTURED | LOCATION |
| 8976 | 1966 | USA |
| PRICE | TOTAL TIME | AVAILABLE |
| $1,200,000 USD | 6,345.5 HRS | 30 Days |

|  |
| --- |
| **AVIONICS** |
| * Single COMM & GPS Garmin GTN-650 |
| * Transponder Bendix KT-76 |
| * Audio panel |

|  |
| --- |
| **EQUIPMENT** |
| * Cargo Hook |
|  |
|  |

**HIGHLIGHTS**

* R/H Tail Rotor

|  |
| --- |
| **INTERIOR** |
| * Troop conﬁguration |
| * New Pilot and copilot seat covers |
|  |













|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Nomenclature | Part Number | Serial No. | TSN | TSO | OH/Life Limit | Life Remaining |
|  |  |  |  |  |  |  |
| Powertrain System |  |  |  |  |  |  |
| Bearing, Hangar | 204-040-623-005 | ND-8441 | 342.3 | \*\*\*\*\* | 1000 | 657.70 |
| Bearing, Hangar | 204-040-623-005 | ND-8629 | 342.3 | \*\*\*\*\* | 1000 | 657.70 |
| Bearing, Hangar | 204-040-623-005 | ND-9316 | 342.3 | \*\*\*\*\* | 1000 | 657.70 |
| Bearing, Hangar | 204-040-623-005 | NE-8262 | 342.3 | \*\*\*\*\* | 1000 | 657.70 |
| Driveshaft, Main | SKCP2281-103 | 1044 | 342.3 | \*\*\*\*\* | COND. | COND. |
| Gearbox, 42' | 212-040-003-023 | AHP-52655 | 2201.9 | 342.3 | 5000 | 4657.70 |
| Gearbox, 90' | 209-040-400-011 | AHV-414 | 2541.0 | 342.3 | COND. | COND. |
| Hangar Assy. | 204-040-600-009 | A20-41904 | \*\*\*\*\* | 342.3 | COND. | COND. |
| Hangar Assy. | 204-040-600-009 | A20-37532 | \*\*\*\*\* | 342.3 | COND. | COND. |
| Hangar Assy. | 204-040-600-011 | A20-13031 | \*\*\*\*\* | 342.3 | COND. | COND. |
| Hangar Assy. | 204-040-600-011 | A20-33627 | \*\*\*\*\* | 342.3 | COND. | COND. |
| Mast Assembly | 204-040-366-015 | A-4221 | 1495.1 | 342.3 | 2500 | 2157.70 |
| Mast Bearing | 212-040-136-001 | JB-0687 | 342.3 | \*\*\*\*\* | 2500 | 2157.70 |
| Mast Pole | 204-011-450-105 | N9-39934 | 342.3 | \*\*\*\*\* | 15000 | 14657.70 |
| Transmission | 205-040-001-017 | B12-309A | 2575.0 | 0 | 2000 | 2000.00 |
| Quill, Main Input | 205-040-263-111 | A12-12680 | 2575.0 | 0 | 2000 | 2000.00 |
|  |  |  |  |  |  |  |
| Miscellaneous |  |  |  |  |  |  |
| Bearing, Turbine Fan Oil Cooler | J33C32 | N/A | 342.3 | \*\*\*\*\* | 450 | 107.70 |
| Bearing, Turbine Fan Oil Cooler | H33C32 | N/A | 342.3 | \*\*\*\*\* | 450 | 107.70 |
| Bolt Kit | 204-1629-2 | N/A | 0 | \*\*\*\*\* | 600 | 600.00 |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| Flight Control System |  |  |  |  |  |  |
| Elevator Horn | 205-001-914-25 | RE-5547 | 558.55 | \*\*\*\*\* | 4800 | 4241.45 |
| Elevator L/H | 205-030-856-019 | ACO-706 | 342.3 | \*\*\*\*\* | 3600 | 3257.70 |
| Elevator R/H | 205-030-856-021 | AS-1386 | 544.55 | \*\*\*\*\* | 3600 | 3055.45 |
| Lever, Collective | 212-010-403-005 | EAFS-12633 | 342.3 | \*\*\*\*\* | COND. | COND. |
| Lever, Collective | 212-010-403-005 | EAFS-12826 | 342.3 | \*\*\*\*\* | COND. | COND. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Nomenclature | Part Number |  | TSN | TSO | OH/Life Limit | Life Remaining |
|  |  |  |  |  |  |  |
| Main Rotor System |  |  |  |  |  |  |
| Blade, Main Rotor | 204P2100-103 | A217 | 0 | \*\*\*\*\* | 2600 | 2600.00 |
| Blade, Main Rotor | 204P2100-103 | A219 | 0 | \*\*\*\*\* | 2600 | 2600.00 |
| Clevis | 204-011-179-001 | A1-05150 | 899 | \*\*\*\*\* | 3600 | 2701.00 |
| Clevis | 204-011-179-001 | A1-10165 | 364 | \*\*\*\*\* | 3600 | 3236.00 |
| Fitting, inboard | 204-012-102-005 | IT-2942 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Fitting, inboard | 204-012-102-005 | IT-3434 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Fitting, outboard | 204-012-103-001 | EAC-5565 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Fitting, outboard | 204-012-103-001 | EAC-5596 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Hub, Main Rotor | 204-012-101-141 | ABG-6538 | 4891.0 | 0 | 2000 | 2000.00 |
| Pin, inboard | 204-012-104-005 | A0-9265 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Pin, inboard | 204-012-104-005 | A0-9266 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Pin, outboard | 204-012-104-005 | A0-9591 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Pin, outboard | 204-012-104-005 | A0-9925 | 1153.0 | \*\*\*\*\* | 2400 | 1247.00 |
| Scissor | 204-011-406-013 | IT-4923 | 342.3 | \*\*\*\*\* | 3600 | 3257.70 |
| Scissor | 204-011-406-013 | IT-4924 | 342.3 | \*\*\*\*\* | 3600 | 3257.70 |
| Scissor's & Sleeve Assembly | 204-011-401-011 | Q19-4810 | 5225.55 | 342.3 | 1200 | 857.70 |
| Stabilizer Bar Centerframe | 204-011-307-001 | 5015A | 342.3 | \*\*\*\*\* | 15000 | 14657.70 |
| Stabilizer Bar Centerframe | 204-011-307-001 | 5015B | 342.3 | \*\*\*\*\* | 15000 | 14657.70 |
| Stabilizer Bar Tube | 212-010-311-101 | SS-02131 | 342.3 | \*\*\*\*\* | COND. | COND. |
| Stabilzer Bar Tube | 212-010-311-101 | EA-265 | 342.3 | \*\*\*\*\* | COND. | COND. |
| Support | 204-011-404-125 | RE-7177 | 342.3 | \*\*\*\*\* | 3600 | 3257.70 |
| Swashplate/Support Assy | 204-011-400-129 | SWFA-5015 | 342.3 | 342.3 | COND. | COND. |
| T.T. Strap | 204-011-122-005 | 37107 | 0 | \*\*\*\*\* | 1200 | 1200.00 |
| T.T. Strap | 204-011-122-005 | 38523 | 0 | \*\*\*\*\* | 1200 | 1200.00 |
| Trunnion Main Rotor | 204-011-105-001 | N/A | 4891.0 | \*\*\*\*\* | 15000 | 10109.00 |
| Yoke, Main Rotor | 204-011-102-017 | IT-0726 | 5462.0 | \*\*\*\*\* | COND. | COND. |
|  |  |  |  |  |  |  |
| Tail Rotor System |  |  |  |  |  |  |
| Slider, Tail Rotor | 204-011-735-003 | \*\*\*\*\* | 342.3 | \*\*\*\*\* | COND. | COND. |
| Tail Rotor Blade | 204-011-702-121 | A-20242 | 516.8 | \*\*\*\*\* | 1200 | 683.20 |
| Tail Rotor Blade | 204-011-702-121 | A-20216 | 413.7 | \*\*\*\*\* | 1200 | 786.30 |
| Tail Rotor Grip | 205-011-711-101 | IT-1340 | 342.3 | \*\*\*\*\* | 2500 | 2157.70 |
| Tail Rotor Grip | 205-011-711-101 | IT-1351 | 342.3 | \*\*\*\*\* | 2500 | 2157.70 |
| Tail Rotor Yoke | 204-011-722-005 | NC-427 | 342.3 | \*\*\*\*\* | 1500 | 1157.70 |
| Tail Rotor Hub Assembly | 204-011-801-017 | Q29-3076 | 342.3 | 342.3 | COND. | COND. |
|  |  |  |  |  |  |  |
| Powerplant System |  |  |  |  |  |  |
| Engine Assembly | T53-L-13B | LE-17912B | 3604.55 | 1078.55 | 2400 | 1321.45 |
| Hot-End Inspection | \*\*\*\*\* | \*\*\*\*\* | \*\*\*\*\* | 342.3 | 1200 | 857.70 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Engine S/N HRS TSN/TSO** | **M/R Blade S/N HRS**  **TSN** | | **M/R Blade S/N HRS**  **TSN** | | **M/R Hub S/N HRS TSN/TSO** | | **T/R Blade S/N HRS**  **TSN** |
| LE-17912B | A217 | | A219 | | ABG-6538 | | A-20242 |
| 3604.55 / 1078.55 | 0.0 | | 0.0 | | 4891.0 / 0.00 | | 516.8 |
| **T/R Blade S/N HRS**  **TSN** | | **Transmission S/N HRS**  **TSN/TSO** | | **(212) 42 Gearbox S/N HRS TSN/TSO** | | **(209) 90 Gearbox S/N HRS TSN/TSO** | |
| A-20216 | | B12-309A | | AHP-52655 | | AHV-414 | |
| 413.7 | | 2575.00 / 0.00 | | 2201.90 / 342.30 | | 2541.00 / 342.30 | |

**ADDITIONAL FEATURES**

* T53-L-13B (-10 Configuration) • ELT
* Hand-Held Fire Extinguisher • GHTI Vertical Fin Spar
* Kaflex Main Driveshaft

**AIRWORTHY AIRCRAFT**

# AIRCRAFT DETAILS

QUOTED CONFIGURATION

**Aircraft Model:** UH-1H

**Engine Model:** T53-L-13B

**USED:** Soundproofing, Battery, Seat Covers, Seat Belts, Fire Extinguisher, Windows

**NEW & USED:** Main Rotor Blades (NEW) & Tail Rotor Blades (USED)

ALL current applicable AD’s, complied with

* **Current Annual Inspection · Dual Flight Controls · 13 Passenger Seating**
* **KAFLEX Main Driveshaft**

OPTIONAL EQUIPMENT:

* **Space Door (Cargo Doors) · Rescue Hoist · 140 gal. Aux. Tank**
* **N1/N2 Engine Cycle Counter · Cabin Wall/Floor Protector · FLIR**
* **CVR/FDR · HUMS · EMS/SAR**
* **HEEL · VIP Seating · Ballistic Protection**
* **Oxygen Mask · Emergency Floats · Tactical Fast Rope System**
* **Air Conditioning · Fire Tank or Bucket · Cabin Protectors**
* **Aerial Spray System · Loud Speakers · Tactical IR/EO Camera Kit**

# AIRCRAFT SPECIFICATIONS DATA

**Aircraft Exterior Dimensions:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Length, fuselage, ft (m)** | **42.40** | **(12.92)** | **Width, fuselage, ft (m)** | **8.00** | **(2.44)** |
| **Length, T/R turning, ft (m)** | **45.93** | **(14.00)** | **Width, widest point, ft (m)** | **9.38** | **(2.86)** |
| **Length, both turning, ft (m)** | **57.28** | **(17.46)** | **Width, landing gear, ft (m)** | **8.67** | **(2.64)** |
| **Height, top, rotor hub, ft (m)** | **13.83** | **(4.210)** | **Gr clearance, fuselage, ft (m)** | **1.00** | **(0.31)** |
| **Height, top, T/R arc, ft (m)** | **16.75** | **(5.100)** | **Gr clearance, T/R, ft (m)** | **5.75** | **(1.75)** |
| **Cabin** |  | **Aircraft Interior Dimensions:** | | **Cabin** |  |
| **Length, max, ft (m)** | **7.67** | **(2.34) Width** | | **8.00** | **(2.44)** |
| **Height, max, ft (m)** | **4.33** | **(1.32) Volume, ft3 (m3)** | | **220.00** | **(6.23)** |

**Aircraft Weights: (Typical)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Max gross, lbs (kg)** | **9,500** | **(4309)** | **Empty, std acft, lbs (kg)** | **5,082** | **(2305)** |
| **Useful load, lbs (kg)** | **4,418** | **(2004)** | **Useful, with full fuel, lbs (kg)** | **1,435** | **(651)** |
| **External load, lbs (kg)** | **4,000** | **(1814)** | **Gross with ext load, lbs (kg)** | **9,500** | **(4309)** |